CARPENTRY TOOL & SAFTEY GEAR (PPE) REQUIREMENTS

The following delineates what the SkillsUSA Virginia Carpentry Technical Committee will provide vs. what is required by the contestant:

1. **Supplied by the technical committee:**
2. Prefabricated sawhorses
3. All lumber and materials, as specified on the job sheet
4. Job sheets and blueprints for each competitor and judge
5. All necessary information and furnishings for judges and technical committee
6. **Supplied by the competitor:**
7. Hardhat
8. Safety Glasses
9. Cut-resistant Level 3 gloves
10. One 8 pt. crosscut saw (10 pt. or 12 pt. optional)
11. Claw hammer
12. Framing square
13. 16’ or longer steel tape measure
14. Utility knife with standard blades
15. Two pencils
16. One each — 1 and 2 pt. Phillips and 4” and 8” standard screwdrivers or one multi-tip with equivalent tip
17. Battery or power operated screw gun for assembling metal framing
18. Ladder- The project will contain roof framing/rafters so bring an OSHA approved ladder or platform
19. Wrecking bar or gooseneck pinch bar
20. Cat’s paw (nail puller)
21. Chalk box and line
22. One nail set
23. Straight aviation snip or any metal-cutting snips
24. 24” or 30” spirit level
25. Combination wood rasp and file (8”)
26. Carpenter’s tool and nail pouch with belt and/or suspenders
27. Stair gauges
28. Combination square and/or speed square
29. 25’ power cord (UL approved grounded)
30. Calculator
31. Power circular saw with new carbide-tipped blade
32. Portable toolbox not to exceed 4.0 cubic feet of storage capacity.